| PrinterUtility_EN 1.1.26

Status

> The main function of this section is to get the current status of the printer.

Status monitoring includes three functions: enabling and disabling printer status queries; viewing printer real-time status data; and viewing printer status records.

Precautions:

1. Before operation, make sure that the port parameters are set correctly and connected to the printer, otherwise the operation is prohibited. Please refer to the "\ref page_1_PortSet" page for port settings.

- Data monitoring operation
  - After the program starts to connect to the device, it enters the status monitoring interface.
  - Click the "Query" button to monitor the status. Red indicates the status bit, the status is active and highlighted. Green indicates that the status bit is not in effect.
  - Move the mouse over the status indicator to display status bit information for that status item.
- Real-time data query operation
  - Click "Data" to view the real-time data byte status information of the printer. The status is on the right and the high position on the left. Green indicates that the bit is 0 and red indicates that the bit is 1.
- Record viewing operation
  - Click "Record" to view the printer status change record.