| PrinterUtility_EN 1.1.26

Printer configuration

> The division mainly contains the following functions:

1. Set up the printer's printing Settings;
2. Switch the usb mode;
3. Query firmware version;
4. Configure the network parameters with usb;
5. Network configuration;
6. Queue Set.

Precautions:

Before operation, make sure that the port parameters are set correctly and connected to the printer, otherwise the operation is prohibited. Please refer to the "\ref page_1_PortSet" page for port settings.

1. The following describes the BK-T680 as an example (different print settings supported by different printer models).

   - Step 1: Go to the printer settings page and select the item you want to set.

     - After the program starts to connect to the device, enter the printer setting interface.
     - Click the Print Settings button.

   - Step 2: Set and save the printer settings 1）Click each drop-down box to select the print settings you want to make. Different printers support different print settings: BTP-R990, BTP-R880NP, BTP-M300 only support setting paper type and density; BT-T080 supports print settings not supported. The BK-T680 supports setting the paper type, density, presenter mode, and presenter wait time. 2）Click the "+" button in the lower left corner to enter the user-defined printer setting interface. The interface is divided into three columns: setting item, instruction and deletion. Click the plus icon to add the customization, double-click the blank to enter the name of the customization printer setting item to be set, and then click the plus icon in the next line to add a new line to set the option name and corresponding instructions. If you want to delete an item, just click the minus sign Icon in the third column. After setting, click the Save button in the lower right corner, and the customized settings will be loaded into the printer setting interface. 3）Click the settings button in the lower right corner to save the current print settings.

2. USB mode switch

   - 1)Click the button to enter the USB mode setting interface. If the current connection mode of the printer is USB, the system will display the USB mode of the currently connected printer. To switch to another USB mode, click the switch button, wait for the following prompt that the conversion is successful, and then restart the printer to make the conversion effective. If the current connection mode of the printer is not USB, the USB mode will not be displayed. Click the switch button Button flyout is not supported.
   - 2）The function is valid only in usb communication, and other communication will remind the function not support.
   - 3）When the printer supports the CDC mode.

3. Query firmware version number

   - 1）Click the firmware version number button to pop up the firmware version number of the currently connected printer when the printer is not connected with parallel port and driver; if the current printer is connected with parallel port or driver, pop-up display is not supported temporarily.
4. Configure the network parameters with usb

   - 1）After entering the usb configuration network interface, the parameter information of the current network board is read from the printer, and the first page is Ad-Hoc mode setting relevant item, the second page is the infrastructure mode setting item.

   - 2）In the mode Ad-Hoc mode, the ssid and password can be configured, and the printer parameters should be restarted after the Settings are set. In the infrastructure mode, all parameters are configurable, and the same restart parameters come into force.
   - 3）If the search is restored by default, all the Settings are restored to the default factory value.

   - 4）The function is valid only in usb communication, and other communication will remind the function not support.

   - 5）All embedded models (such as the BK series of BT series printers) will not be able to hold this function, and will also be a warning to the function.
5. Network configuration

   - 1）Clicking the network configuration button will launch the BYNetConfig configuration tool, which mainly searches and configures network interface devices within the local area network through the UDP broadcast protocol. It supports multiple network card searches, and specific functions can be found in the tool's help document.

6. Queue set

   - 1）Click the queue set to set whether to enable the queue function, set the initial value, the number of copies, the date, the text, etc.You can choose whether to set date.
   - 2）When the setting is completed, you can print as shown in the following figure by pressing the paper feed key of the printer, press once to print once, and the serial number is incremented.

Precautions:

1. When the printer is BK-T680, the presenter wait time can be set only when the presenter mode selects "presenter open, retract", "continue, retract (file send)", "continue, retract (file hold)".
2. The printer settings may not be valid when you print your own samples.