| PrinterUtility_EN 1.1.26

CodePage

> The main function of this part is to create, open, edit, save, download, query, print and other operations on the code page.

The code page includes the following nine functions: select the enable code page; create a new code page; open the code page; edit the code page; save the code page; download the code page; query the downloaded code page information; clear the downloaded code page; print and Set the default code page.

Precautions:

1. Before operation, make sure that the port parameters are set correctly and connected to the printer, otherwise the operation is prohibited. Please refer to the "\ref page_1_PortSet" page for port settings.

- Enable code page

  - Select code page type
    - Code page
    - User-defined character
  - Enable code page
- New code page
  - Character type rate
    - 9x10
    - 9x12
    - 9x17
    - 12x24
    - 13x24
    - 18x34
  - The dot matrix printer generally supports 9x10 and 9x12 thermal printers: 200dpi supports 9x17 and 12x24, and 300dpi supports 13x24 and 18x34.

- Open code page

- Edit code page

  - First open the code page file or create a new code page file
  - Check a character
  - Edit character
- Save code page

- Download code page

  - Select area ID
  - Select code ID
  - Note: The new version of the firmware ignores the area ID.

- Query information about downloaded code pages

  - The information showing each area contains the code number and font number.

- Clear downloaded code page

  - Clear downloaded code page and clear regional status table

- Print and set the default code page

  - Print downloaded code page
  - Select Print Code Page as Default Code Page

- After editing the code page, saving it, creating, opening, or closing the program will prompt you if you need to save the code page.