| PrinterUtility_EN 1.1.26

Samples

> The main function of this section is to print a variety of different types of proofs.

The sample print includes four special examples and other examples: an example display; a watermark example; a nested example; a custom example; other examples.

Precautions:

1. Before operation, make sure that the port parameters are set correctly and connected to the printer, otherwise the operation is prohibited. Please refer to the "\ref page_1_PortSet" page for port settings.
2. The following describes the BK-T680 as an example (there are different types of examples supported by different printer models).

- Sample display

  - The program starts to connect to the device and enters the sample print interface.
  - The examples shown in the program interface are all examples configured in the xml file, and the examples of switching models are different.

- Watermark example

  - Before printing the watermark example, select a bitmap to be downloaded into the printer in the bitmap printing interface as the watermark image (only the monochrome bitmap is stored in the flash).
  - Watermark parameter configuration: modify the watermark parameter, select the downloaded bitmap number, click the save button, the watermark parameter is saved; the print button is enabled, and the watermark sample is printed when clicked (the watermark parameter will be invalid after the printer is restarted).

- Chromato

  - The data table shows the data items that are hollow out of the current template and what needs to be filled out.
  - Click the download button to download the prepared template to the printer. The Print button and the Cut check box are enabled. Click the Print button to print the edited content in the data table to the blank data location in the template.

- User Define

  - Click the Customize Sample button, a pop-up dialog box will select the sample file, and click Open to directly print the selected sample file.
- Other examples
  - In addition to the above examples that require special editing, other examples simply print the sample samples by clicking the button.